; Copyright (c) 2009-2012 Intel Corporation 
; ********************************************************************************************** 
; ********************************************************************************************** 
; **    Filename:  iaStorS.inf 
; **    Revision:  10/18/2012,3.6.0.1086 
; **    Abstract:  Windows* INF File for SCU Intel(R) Rapid Storage Technology Enterprise Driver 
; **               Installs: RSTe SCU RAID Controller Miniport + RST Filter Driver 
; ********************************************************************************************** 
; 
[Version] 
Signature = "$Windows NT$" 
Class=SCSIAdapter 
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318} 
Provider=%INTEL% 
CatalogFile=iaStorS.cat 
DriverVer=10/18/2012,3.6.0.1086
; 
[PackageInfo] 
Name=SCU 
; 
[SourceDisksNames] 
1 = %DiskId1%,,,"" 
; 
[DestinationDirs] 
DefaultDestDir = 12 
; 
[ControlFlags] 
ExcludeFromSelect = * 
; 
[Manufacturer] 
%INTEL% = INTEL, NTx86.5.2, NTamd64 
; 
[Intel_SCU_iaStorS_Service_Inst] 
ServiceType    = %SERVICE_KERNEL_DRIVER% 
StartType      = %SERVICE_BOOT_START% 
ErrorControl   = %SERVICE_ERROR_NORMAL% 
ServiceBinary  = %12%\iaStorS.sys 
LoadOrderGroup = SCSI Miniport 
AddReg         = pnpsafe_pci_addreg 
AddReg         = UserParameters 
;AddReg         = msienable_addreg 
; 
[Intel_SCU_EventLog_Inst] 
AddReg = Intel_SCU_EventLog_Inst.AddReg 
; 
[Intel_SCU_EventLog_Inst.AddReg] 
HKR,,EventMessageFile,%REG_TYPE_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorS.sys" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7 
; 
[iaStorF_Service_Inst] 
ServiceType    = %SERVICE_KERNEL_DRIVER% 
StartType      = %SERVICE_BOOT_START% 
ErrorControl   = %SERVICE_ERROR_NORMAL% 
ServiceBinary  = %12%\iaStorF.sys 
; 
[iaStorF_EventLog_Inst] 
AddReg = iaStorF_EventLog_AddReg 
; 
[iaStorF_EventLog_AddReg] 
HKR,,EventMessageFile,%REG_TYPE_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7 
; 
;****************************************************************************** 
;* 
;* 32-BIT X86 ARCHITECTURE 
;* 
;* This section specifies the 32-bit architecture specific INF file entries 
;* required to install a driver as a 32-bit compatible driver. 
;* 
;****************************************************************************** 
[SourceDisksFiles.x86] 
iaStorS.sys = 1,,, 
iaStorF.sys = 1,,, 
; 
[INTEL.NTx86.5.2] 
;;; SCU 0 Device IDs 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D60 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D61 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D64 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D65 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D68 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D69 
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6A 
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6B 
; 
[Intel_SCU_iaStorS_Inst.NTx86] 
CopyFiles = @iaStorS.sys 
CopyFiles=@iaStorF.sys 
; 
[Intel_SCU_iaStorS_Inst.NTx86.HW] 
AddReg = iaStorF_addreg 
AddReg = msienable_addreg 
AddReg = storport_addreg 
Include = machine.inf 
Needs = PciIoSpaceNotRequired 
; 
[Intel_SCU_iaStorS_Inst.NTx86.Services] 
AddService = iaStorS,%SPSVCINST_ASSOCSERVICE%,Intel_SCU_iaStorS_Service_Inst, Intel_SCU_EventLog_Inst 
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst 
; 
;****************************************************************************** 
;* 
;* 64-BIT X86 ARCHITECTURE 
;* 
;* This section specifies the 64-bit architecture specific INF file entries 
;* required to install a driver as a 64-bit compatible driver. 
;* 
;****************************************************************************** 
[SourceDisksFiles.amd64] 
iaStorS.sys = 1,,, 
iaStorF.sys = 1,,, 
; 
[INTEL.NTamd64] 
; 
;;; SCU Device IDs 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D60 
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D61 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D62 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D63 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D64 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D65 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D66 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D67 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D68 
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D69 
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6A 
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6B 
; 
[Intel_SCU_iaStorS_Inst.ntamd64] 
CopyFiles = @iaStorS.sys 
CopyFiles=@iaStorF.sys 
; 
[Intel_SCU_iaStorS_Inst.ntamd64.HW] 
AddReg = iaStorF_addreg 
AddReg = msienable_addreg 
AddReg = storport_addreg 
Include = machine.inf 
Needs = PciIoSpaceNotRequired 
; 
[Intel_SCU_iaStorS_Inst.ntamd64.Services] 
AddService = iaStorS,%SPSVCINST_ASSOCSERVICE%,Intel_SCU_iaStorS_Service_Inst, Intel_SCU_EventLog_Inst 
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst 
; 
;****************************************************************************** 
;* 
;* RST FILTER Driver REGISTRY CHANGES 
;* 
;* This section specifies the registry entries necessary to add the lower disk 
;* class RST Filter driver.  Layer the RST Filter driver under all Disk class 
;* GUID devices as a lower disk class filter.. 
;* 
;****************************************************************************** 
[iaStorF_addreg] 
HKLM, System\CurrentControlSet\Control\Class\{4d36e967-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF 
; 
;****************************************************************************** 
;* 
;* PLUG-N-PLAY REGISTRY CHANGES 
;* 
;* This section specifies the registry entries necessary to indicate support 
;* for Plug-n-Play. 
;* 
;****************************************************************************** 
[pnpsafe_pci_addreg] 
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001 
; 
; BusType 0xA == BusTypeSas (winioctl.h) 
; PCI subclass code indicates SAS (not RAID), so for WHQL, the BusType 
;  needs to match 
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x0000000A 
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001 
;****************************************************************************** 
;* 
;* MSI/MSI-X REGISTRY CHANGES 
;* 
;* This section specifies the registry entries necessary in order to indicate 
;* this driver supports MSI-X. 
;* 
;****************************************************************************** 
[msienable_addreg] 
;;;  Indicate we support MSIx up to 2 message vectors 
;HKR, Interrupt Management,                                    ,                   %REG_TYPE_KEY_ONLY% 
HKR, Interrupt Management, 0x00000010 
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010 
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1 
[storport_addreg] 
;;; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255) 
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF 
;****************************************************************************** 
;* 
;* USER PARAMETER REGISTRY CHANGES 
;* 
;* This section specifies the parameters that users can modify in the 
;* registry that will change the operation of the driver after a power 
;* cycle of the system or a reinstall of the driver. 
;* 
;****************************************************************************** 
[UserParameters] 
;;; Build the Registry Directories 
HKR, Parameters, Device, %REG_TYPE_KEY_ONLY% 
; 
;;; Add the RAID features 
HKR, Parameters\Device, ReadPatrol,                               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, RebuildOnHotInsert,                       %REG_TYPE_BINARY%,     0x00000000 
; 
;;; Add the Controller wide user parameters 
HKR, Parameters\Device, ControllerDeviceSpinUpDelayInterval,      %REG_TYPE_DWORD%,      0x000001F4 
HKR, Parameters\Device, ControllerInterruptCoalescenceNumber,     %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, ControllerInterruptCoalescenceTimer,      %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, ControllerSataNcqEnable,                  %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, ControllerSataNcqDepthMaximum,            %REG_TYPE_DWORD%,      0x00000020 
HKR, Parameters\Device, ControllerSataStandbyTimerEnable,         %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, ControllerSataNonZeroBufferOffsetEnable,  %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, ControllerInitialResetType,               %REG_TYPE_DWORD%,      0x00000008 
HKR, Parameters\Device, ControllerClearAffiliationEnable,         %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, StpInactivityTimeout,                     %REG_TYPE_DWORD%,      0x00000005 
HKR, Parameters\Device, SspInactivityTimeout,                     %REG_TYPE_DWORD%,      0x00000005 
HKR, Parameters\Device, StpMaxOccupancyTimeout,                   %REG_TYPE_DWORD%,      0x00000005 
HKR, Parameters\Device, SspMaxOccupancyTimeout,                   %REG_TYPE_DWORD%,      0x00000014 
HKR, Parameters\Device, NoOutBoundTaskTimeout,                    %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, IgnoreFUA,                                %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, PerformanceOptimizationsEnable,           %REG_TYPE_DWORD%,      0x00000000 
; 
HKR, Parameters\Device, InterruptCoalescingSampleSize,      %REG_TYPE_DWORD%,      0x0000000a 
HKR, Parameters\Device, InterruptCoalescingSampleFrequency, %REG_TYPE_DWORD%,      0x00000064 
HKR, Parameters\Device, InterruptCoalescingThreshold,       %REG_TYPE_DWORD%,      0x00002800 
HKR, Parameters\Device, InterruptCoalescingLowNumber,       %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, InterruptCoalescingLowTimeout,      %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, InterruptCoalescingHighNumber,      %REG_TYPE_DWORD%,      0x00000010 
HKR, Parameters\Device, InterruptCoalescingHighTimeout,     %REG_TYPE_DWORD%,      0x00000002 
; 
;;; Add the Phy specific user parameters 
HKR, Parameters\Device, Phy0NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033 
HKR, Parameters\Device, Phy0AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f 
HKR, Parameters\Device, Phy0InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff 
HKR, Parameters\Device, Phy1NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033 
HKR, Parameters\Device, Phy1AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f 
HKR, Parameters\Device, Phy1InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff 
HKR, Parameters\Device, Phy2NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033 
HKR, Parameters\Device, Phy2AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f 
HKR, Parameters\Device, Phy2InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff 
HKR, Parameters\Device, Phy3NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033 
HKR, Parameters\Device, Phy3AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f 
HKR, Parameters\Device, Phy3InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff 
HKR, Parameters\Device, Controller0Phy0MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller0Phy1MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller0Phy2MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller0Phy3MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller1Phy0MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller1Phy1MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller1Phy2MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
HKR, Parameters\Device, Controller1Phy3MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002 
; 
;;; Add the Port specific OEM parameters 
HKR, Parameters\Device, OemHeaderVersion,                         %REG_TYPE_DWORD%,      0x00000010 
HKR, Parameters\Device, Controller0OemModeType,                   %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemConcurrentDeviceSpinUpCount,%REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemSscEnable,                  %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller0OemPort0PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller0OemPort1PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller0OemPort2PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller0OemPort3PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller0OemPhy0SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemPhy0SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller0OemPhy1SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemPhy1SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller0OemPhy2SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemPhy2SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller0OemPhy3SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller0OemPhy3SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
; 
HKR, Parameters\Device, Controller1OemModeType,                   %REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller1OemConcurrentDeviceSpinUpCount,%REG_TYPE_DWORD%,      0x00000001 
HKR, Parameters\Device, Controller1OemSscEnable,                  %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller1OemPort0PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller1OemPort1PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller1OemPort2PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller1OemPort3PhyMask,               %REG_TYPE_DWORD%,      0x00000000 
HKR, Parameters\Device, Controller1OemPhy0SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004 
HKR, Parameters\Device, Controller1OemPhy0SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller1OemPhy1SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004 
HKR, Parameters\Device, Controller1OemPhy1SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller1OemPhy2SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004 
HKR, Parameters\Device, Controller1OemPhy2SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller1OemPhy3SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004 
HKR, Parameters\Device, Controller1OemPhy3SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF 
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08 
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069 
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09 
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E 
HKR, Parameters\Device, BackplaneIsPassive,                       %REG_TYPE_DWORD%,      0x00000000 
;****************************************************************************** 
;* 
;* INF FILE STRINGS (VARIABLES) 
;* 
;* This section specifies variables that can be reused elsewhere in this 
;* INF file. 
;* 
;****************************************************************************** 
[Strings] 
;;;  *******Localizable Strings******* 
diskId1                = "iaStorS Installation Disk" 
Intel_SAS_RAID.Desc    = "Intel(R) C600 Series Chipset SAS RAID Controller" 
Intel_SATA_RAID.Desc   = "Intel(R) C600 Series Chipset SAS RAID (SATA mode)" 
INTEL = "Intel Corporation" 
; 
;;;  *******Non Localizable Strings******* 
SERVICE_BOOT_START     = 0x0 
SERVICE_SYSTEM_START   = 0x1 
SERVICE_AUTO_START     = 0x2 
SERVICE_DEMAND_START   = 0x3 
SERVICE_DISABLED       = 0x4 
SERVICE_KERNEL_DRIVER  = 0x1 
; 
SERVICE_ERROR_IGNORE   = 0x0 
SERVICE_ERROR_NORMAL   = 0x1 
SERVICE_ERROR_SEVERE   = 0x2 
SERVICE_ERROR_CRITICAL = 0x3 
; 
REG_TYPE_BINARY    = 0x00000001 
REG_TYPE_KEY_ONLY  = 0x00000010 
REG_TYPE_DWORD     = 0x00010001 
REG_TYPE_EXPAND_SZ = 0x00020000 
; 
SPSVCINST_ASSOCSERVICE = 0x00000002 
