[fx-9860G Emulator Function Reference]           Sep.22.2005      CASIO COMPUTER CO., LTD. 

1)Special Keys

PC Key         Emulator Function
---------------------------------------
[Tab]           [AC]
[Insert]        [SHIFT]
[Home]          [OPTN]
[PageUp]        [VARS]
[PageDown]      [MENU]
[End]           [ALPHA]
[Esc]           [EXIT]
[Delete]        [DEL]
[Back]          [DEL]
[Enter]         [EXE]
[F1] - [F6]     [F1] - [F6]
[F12]           Screen capture (bitmap file)



2)Shortcut Menu
Right-clicking with the mouse displays a shortcut menu with the following commands. 

-Popup Display
Displays the screen on a popup window from 2X to 6X normal size. 

-Screen to Folder 
Displays a dialog box for specifying a file name and folder for storage of screen captures
created with the [F12] function key. 

-Automatic Capture Screen
Configures the computer to assign serial numbered file names to BMP files of screen captures
created with the [F12] function key. Files are stored in the folder that it initially specified. 

-Caps Lock
Uses upper case characters for all alphabetic input on the PC keyboard. 
It is probably best to turn this option off when creating an eActivity. 

-Copy
Copies the selected area when using the emulator's Clip function. 
The area also is copied simultaneously to the PC's clipboard.*1

-Paste
Pastes the PC's clipboard contents into the emulator.*1
Note however that this command is enabled only in cases where the emulator's Paste
command ([SHIFT] [9]) can be performed. 

-Capture Screen
Copies the current display to the PC's clipboard. The same function can be performed
by pressing the emulator's [F-D] key. 

-About
Displays the emulator version. 

-Exit
Exits the emulator. 

*1:Non-ASCII code characters cannot be displayed properly. 
Characters of "+"/"-" keys on the emulator cannot be displayed properly too.



*** Precautions *** 
The function that allows the calculator to access an SD card is used by the emulator to access the PC.
Data can be saved on the PC and then loaded from the PC. 

Note, however, that the location being accessed on the PC should be a local PC writable hard disk. 
Any other type of device can cause malfunction. 


In no event shall CASIO Computer Co., Ltd. be liable to anyone for special, collateral, incidental,
or consequential damages in connection with or arising out of the purchase or use of these
materials. Moreover, CASIO Computer Co., Ltd. shall not be liable for any claim of any kind
whatsoever against the use of these materials by any other party.





[System Requirements]
CPU:               Minimum required Intel(R) Pentium(R)3  800MHz
                   Recommended Intel(R) Pentium(R)4  2.4GHz or higher
Operating Systems: Windows(R) 2000/XP
Disk Space:        10MB
Memory:            128MB
Video Display:     1024*768  High Color(16 bit) or higher



*** Note ***
Company and product names used herein are trademarks of their respective owners.
